Cross punisher part 2



1. One of my lovely friends has a husband with a garage filled with power tools that came in handy while cutting these out. I used a jig saw to cut out the crosses and a rotary saw and a scroll saw to cut out the wooden piece. Afterward there is still a lot of sanding to make the correct shape.
2. The wooden piece is the trigger/handle. The two small cross arm pieces will be attached later.



1.  The worse part of this project was carving out the space on the underside of the crosses for the trigger/handle. I used a dremel rotary tool. It is important to cut this space a depth of half the thickness of your trigger/handle. You do not want there to be a lot of wiggle room, you want a tight fit. Repeat this process on the second cross. Test the fit before you glue. 🡺🡺🡺